1. **COFFERDAMS (Revised 3-21-03)**

Description. Enclose all substructure construction in the active streambed in a wall type cofferdam. Have an engineer that is registered in Montana approve the cofferdam design.

Submittals. Submit two copies of the design calculations and four copies of the stamped and signed drawings to the Project Manager for approval. Do not begin construction of any cofferdam prior to receiving approval.

Consider cofferdams temporary facilities for the requirements of Subsections 107.11 and 208.03 of the Standard Specifications.