**405-3 Crack Sealant Removal Prior to Cold Recycle (Revised 10-24-19)**

**(Use only when CIPR operations will be followed by Seal Coat only)**

1. CRACK SEALANT REMOVAL PRIOR TO COLD RECYCLE [405] (REVISED 10-24-19)

Description. The work is removing crack sealant materials from the roadway prior to initiating Cold Recycle operations.

Materials. Vacant.

Construction Requirements. Remove all crack sealant and backer rod from the roadway prior to beginning milling operations. Fully remove all crack sealant materials from the depth of the roadway to be recycled. Dispose of the material to the satisfaction of the Project Manager.

Method of Measurement. Crack sealant removal is not measured separately for payment.

Basis of Payment. Crack sealant removal is included in the contract unit price for Cold Recycled Plant Mix and is not paid for separately.