1. IMPACT ATTENUATOR [606] (REVISED 9-11-14)

Install a Test Level 3, CHOOSE SIZE wide impact attenuator at the location shown in the plans. The device must be rated for 60 mph (100 kph) and conform to the detail drawings.

Obtain complete detailed drawings and material costs for construction and bidding purposes from the manufacturer. Install the impact attenuator in accordance with manufacturer's specifications. Use Class General concrete, following the requirements of Subsection 551.03.2, for the required concrete pad.

Ensure existing concrete pad meets manufacturer’s specifications if replacing existing impact attenuator.

Do not remove the existing guardrail until the impact attenuator is at the project site, and has been inspected and approved for use by the Project Manager.

Measurement and payment will be at the contract unit price per each, which includes all materials, labor and equipment to install complete in place.