1. Concrete Warranty [608] (added 4-23-20)

Concrete sidewalk, curb and gutter, median curb, and median cap are subject to a 1-year performance warranty.

The Project Manager has sole authority to determine concrete performance following the 1-year warranty period. The 1-year warranty period starts on the date of the completion of the final concrete placement in each calendar year and ends one year from that defined date. The Project Manager will give written notice to the Contractor of the beginning of the warranty period.

Defective concrete is defined as the presence of scaling, cracking, pop-outs, spalling, or any other deficiency identified by the Project Manager. Deficient Concrete is referenced in the Department’s Concrete Warranty Administration Guide. The Project Manager will notify the Contractor in writing of observed deficiencies that occur within the warranty period. Submit a detailed repair plan to the Project Manager within 14 calendar days of the notification of required repairs.

Damage from Department or local maintenance activities, vandalism or other causes beyond the control of the Contractor is not subject to the warranty.

Replace deficient concrete to the nearest contraction joint or as approved in the repair plan. Acceptance of repair work will be in accordance with Subsection 105.03.1. Restore pavement markings and furnish traffic control at no additional cost to the Department.

Complete warranty work within 30 calendar days of the approved repair plan unless otherwise approved in writing by the Project Manager.